**2800 Catamaran Boat and Passenger boat**

|  |  |  |  |
| --- | --- | --- | --- |
| **verall Length(inc.fishing platfor** | 28m | overall width | 6.5m |
| waterline | 23.91m | twin bottom |  |
| beam |  | depth | 2.35m |
| draft | 1m | displacement | 36.26t |
| engine(Cummins) | 2x450hp | speed | 21kn |
| seats | 150xseats in cabin | cruising | 200nm |
| navigation area | coastal | load 200persons |  |

Prices Include Global Shipping: US$1,130,000.00/yacht (2x450HP Cummins) USD980,000.00/boat (2x455HP international inboard diesel )

**Main Eqiupment List**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **No.** | **Item** | **Specification/Model** | **Qua ntity** | **Remark** |
| **一** | **FRP Project** | **gel coat、resin、glass fiber materials are approved by**  **marine inspection** | | |
| **二** | **fitting&decoration** |  | | |
| **1** | **instrument panel** | **cherry wood on FRP console** | **1set** | **China** |
| **2** | **driver seat** | **adjustable aluminum alloy super seat and safe belt** | **2** | **China** |
| **3** | **passenger seats** | **aluminum alloy support seats** | **140** | **China** |
| **4** | **multi-funtion room** | **inc.leather-imitate sofa,tea table** | **1** | **China** |
| **5** | **Driver cabin ceiling** | **synthetic hide** | **1set** | **China** |
| **6** | **front&back cabin ceiling** | **synthetic hide** | **1set** | **China** |
| **7** | **side wall** | **red cherry board** | **1set** | **China** |
| **8** | **floor** | **plywood or carpet** | **1set** | **China** |
| **9** | **fixed window for diiver cabin** | **archy toughened glass** | **1set** | **China** |
| **10** | **porthole** | **aluminum alloy tougheded glass window** | **1set** | **China** |
| **11** | **sliding door** | **natural wood(bedroom)** | **2sets** | **China** |
| **12** | **sliding door** | **teak (passenger cabin)** | **1set** | **China** |
| **13** | **public toilet** | **squat toilet,shouwer** | **1set** | **China** |
| **15** | **sightseeing top** | **inc.FRP chairs,tea table** | **1set** | **China** |
| **16** | **luxurious curtain** |  | **1set** | **China** |
| **17** | **rain wiper** |  | **1set** | **imported** |
| **18** | **fresh water tank** | **1000×600×400mm** | **1** | **China** |
| **19** | **rails,bollard,lifting ring,ladder for** | **s/s、rail height:900mm** | **1set** | **China** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **20** | **windscreen** | **toughened glass** | **1set** | **China** |
| **21** | **anti-collision ball** | **rubber** | **1set** | **China** |
| **三、motor** | | | | |
| **1** | **engine** | **2x450hp** | **2** | **Cummins** |
| **2** | **gear case** | **HC200** | **2** | **China** |
| **3** | **axles** | **316L S/S** | **1set** | **China** |
| **4** | **seal lubricating** |  | **1set** | **China** |
| **5** | **screw propeller** | **manganese-alumnum bronze** | **2** | **China** |
| **6** | **steering system** |  | **1set** | **France** |
| **7** | **rudder indicator** | **VOD** | **1set** | **Germany** |
| **8** | **fuel tank** | **steel, with fuel level gauge** | **2** | **China** |
| **9** | **oil&water seperator** | **0.05 cubic** | **1** | **China** |
| **10** | **fire alarm** |  | **1set** | **China** |
| **11** | **muffler** |  | **2** |  |
| **12** | **vent-pipe** |  | **2** |  |
| **13** | **hand-sway pump** | **CS25\CS-32** | **各1** |  |
| **14** | **fuel pump** |  | **1** |  |
| **15** | **electric firefighting** |  | **1** |  |
| **16** | **instruments** |  | **1set** |  |
| **17** | **pipeline** |  | **1set** |  |
| **18** | **valves** |  | **1set** |  |
| **19** | **sound insulation cotton in motor cabin** |  | **1set** |  |
| **20** | **motor room exhaust system** |  | **1set** |  |
| **四、electricity&gas** | | | | |
| **1** | **generator unit** | **24kw,220V** | **1** | **China** |
| **2** | **generator unit** | **5kw,220V** | **1** | **China** |
| **3** | **air conditioner** | **220V,36000BTU** | **2** | **China** |
| **4** | **charger** | **SCR-HF25A12-24V** | **1** | **China** |
| **5** | **main electric board** |  | **1set** | **China** |
| **6** | **storage battery** | **6-Q-195Model-12V.24V** | **7** | **China** |
| **7** | **shore electric box** |  | **1set** | **China** |
| **8** | **electricity charge&discharge** |  | **1set** |  |
| **9** | **radar** | **JRC2343** | **1** | **Japan** |
| **10** | **VHF phone** | **VHF7100** | **1** | **New Zealand** |
| **11** | **satellite positioning** | **GPS168** | **1** | **Japan** |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **12** | **radar search responder** | **RT-10** | | **1** | **Korea** |
| **13** | **AIS auto identifying system** | **AIS-108** | | **1** | **Korea** |
| **14** | **VHF bi-directional wireless phone** | **TW-50** | | **2** | **Korea** |
| **15** | **depth sounder** | **FISH4300** | | **1** | **New Zealand** |
| **16** | **navigation alarm receiver** |  | | **1** | **Japan** |
| **17** | **electric anchor motor** | **Aries1400D-24V** | | **1** | **France** |
| **18** | **temperature&smoke inductor** | **JTY-ZD** | | **1set** |  |
| **19** | **search light** | **SL135** | | **1** | **America** |
| **20** | **loudspeaker** |  | | **1set** |  |
| **21** | **media facilities** | **disc player,amplifier system,acoustics(multifunction** | | **1set** | **China** |
| **22** | **LC TV** | **one of 32",two of 20 "** | | **3** | **China** |
| **23** | **DVD for cars** | **host&guest room** | | **2** |  |
| **24** | **steam siren** |  | | **1** |  |
| **25** | **navigation signal** | **24V、25W** | | **1set** |  |
| **26** | **cabin lights** |  | | **1set** |  |
| **27** | **lightning system** |  | | **1set** |  |
| **28** | **inverter** |  | | **1** |  |
| **29** | **magnetic compass** |  | | **1** |  |
| **30** | **clinometer** |  | | **1** |  |
| **五、** | **other accessories with boat** | | | | |
| **1** | **sea boat life jacket** |  | **32pcs** | | |
| **2** | **child life jacket** |  | | **6** |  |
| **3** | **sea boat buoy** | **two with auto buoy light,the other two with 30m life saving buoy rope** | | **4** |  |
| **4** | **inflatable lifesaving raft for 15 persons** |  | | **2** |  |
| **5** | **fire figthing barrel** |  | | **4** |  |
| **6** | **fire fighting facilities** | **fire hydrant,water hose and squirt gun** | | **1set** |  |
| **7** | **fire extinguisher** | **4kg** | | **2** |  |
| **8** | **fire extinguisher** | **2Kg** | | **6** |  |
| **9** | **fire extinguisher** | **24Kg** | | **1uni** |  |
| **10** | **yellow sandbox** |  | | **4** |  |
| **11** | **axe** |  | | **1** |  |
| **12** | **rocket parachute** |  | | **12** |  |

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **13** | **telescope** |  | **1** | |  | |
| **14** | **bell** |  | **1** | |  | |
| **15** | **signal flag** |  | **1set** | |  | |
| **16** | **anchor** | **s/s** | **1** | |  | |
| **17** | **anchor rope** | **Ф26mm** | **50m** | |  | |
| **18** | **无档anchor chain** | **Ф1.10mm** | **5m** | |  | |
| **19** | **rope** | **length:50mm** | **3** | |  | |
| **20** | **tools** |  | **1set** | |  | |
| **21** | **inspection certificate** |  | **1set** | |  | |
| **22** | **qualified certificate** | | | **1** | |  |
| **23** | **technical documents** | | | **1set** | |  |
|  | | | | | | |

****





